


1. Copy MIB file to PC service。
2. Login SNMP，set Authorized IP Address，in Authorization select Readable/Writeable




1. Run mib browser，enter IP of SNMP




4, Load mib file, click load MIBs, select mib file to load




5、Right click the mib loaded，select walk.





6、Now，user can see UPS data of mib



Noise：

If you not in SNMP card web setting Authorization,it will be tip error:

